For Q.36, I was able to get to the point where table 12 is, but not able to decide which column I should use between 2 and 3 current carrying conductors. What is the keyword to decide this in this question or is it trade knowledge?

Can check the answer for Q89? I went to the code 12-3012(2) but it looks different with the answer.